--lpm_add_sub CARRY_CHAIN="MANUAL" CARRY_CHAIN_LENGTH=48 DEVICE_FAMILY="Cyclone IV GX" LPM_PIPELINE=0 LPM_REPRESENTATION="SIGNED" LPM_WIDTH=6 ONE_INPUT_IS_CONSTANT="YES" cin dataa datab result
--VERSION_BEGIN 14.1 cbx_cycloneii 2014:12:03:18:04:04:SJ cbx_lpm_add_sub 2014:12:03:18:04:04:SJ cbx_mgl 2014:12:03:18:06:09:SJ cbx_stratix 2014:12:03:18:04:04:SJ cbx_stratixii 2014:12:03:18:04:04:SJ  VERSION_END


-- Copyright (C) 1991-2014 Altera Corporation. All rights reserved.
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, the Altera Quartus II License Agreement,
--  the Altera MegaCore Function License Agreement, or other 
--  applicable license agreement, including, without limitation, 
--  that your use is for the sole purpose of programming logic 
--  devices manufactured by Altera and sold by Altera or its 
--  authorized distributors.  Please refer to the applicable 
--  agreement for further details.



--synthesis_resources = lut 6 
SUBDESIGN add_sub_pmh
( 
	cin	:	input;
	dataa[5..0]	:	input;
	datab[5..0]	:	input;
	result[5..0]	:	output;
) 
VARIABLE
	result_int[6..0]	:	WIRE;
BEGIN 
	result_int[] = (dataa[], cin) + (datab[], cin);
	result[] = result_int[6..1];
END;
--VALID FILE
